1 Footing total dimensions to be given (0:No, 1:Yes)
0 Footing break-up dimensions to be given (0:No, 1:Yes)
1 Column total dimensions to be given (0:No, 1:Yes)
0 Column break-up dimensions to be given (0:No, 1:Yes)
0 Wall footing & Column Footing Crossing to be checked (0:No, 1:Yes)
1 DecaPlot sheet border
0 Grid lines, marks, dimensions & columns to be drawn (0:No, 1:Yes)
1 Footing & pedestals to be drawn (0:No, 1:Yes)
0 Walls (without wall footing lines) to be drawn (0:No, 1:Yes)
1 Wall footing lines to be drawn (0:No, 1:Yes)
0 Wall mark writing option (0:All spans, 1:Once between left & right wall, 2:Once for same thickness wall)
0 BBS required (0:No, 1:Yes)
0 BBS on A4 size sheets required (0:No, 1:Yes)
25 Mix for Laps
0 Footing schedule (0:No, 1:Yes)
0 Kink Option (0:No Kink, 1:Auto Kink)
1 Links as per IS:13920 (0:No, 1:Yes)
0 Full Height Title Block
1 Dimension between Ground Level & Bottom of P.C.C.
0 Links X-Sectional Area as per IS:13920 (0:No, 1:Yes)
500 fy
0 F1, F2, F3
1 Isolated & User Specified Combined Foundations
0 No Red Cross on failing columns/ foundations
